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Features

M High surge current capability

W Stud cathode and stud anods version
W Wide current range

™ Matric device version available

Typical Applications

m Battery charges Ordering Information Table

=

W Machine tool controls
WWelder M Motor controls

~None=Standard recovery dodes;
FR=Fast recovery diodes

i -Gurtent code=IFy,

Polarity -Outline code: F=D0-4 case 6A-25A; HF=
U=D0-8,00-9 case 100A-300A
~None=Stud Normal Polaity (cathode to stud)
R=Stud Reverse Polarity (anode fo stuc)
Votags code=coda x 10=Vmu
-None=Standrd nch Devics; M=Mstric Device
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Normal Reverse

0-5 case 30A-85A

ELECTRICAL CHARACTERISTICS
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